PCBNEW-BOARD Version 1 date 2013-11-19 08:30:06

# Created by Pcbnew(2012-01-19 BZR 3256)-stable

$GENERAL
encoding utf-8
LayerCount 2
Ly 1FFF8001
EnabledLayers 1FFF8001
Links 23
NoConn 1
Di 21002 7849 34040 20380
Ndraw 6
Ntrack 46
Nzone 0
BoardThickness 630
Nmodule 13
Nnets 9
$EndGENERAL

$SHEETDESCR
Sheet A4 11700 8267
Title ""
Date "19 nov 2013"
Rev ""
Comp ""
Comment1 ""
Comment2 ""
Comment3 ""
Comment4 ""
$EndSHEETDESCR

$SETUP
InternalUnit 0.000100 INCH
Layers 2
Layer[0] Dolna signal
Layer[15] Gorna signal
TrackWidth 102
TrackWidthList 102
TrackWidthList 197
TrackWidthList 394
TrackWidthList 591
TrackWidthList 791
TrackWidthList 1185
TrackWidthList 1382
TrackClearence 100
ZoneClearence 0
TrackMinWidth 98
DrawSegmWidth 150
EdgeSegmWidth 150
ViaSize 350
ViaDrill 250
ViaMinSize 350
ViaMinDrill 200
MicroViaSize 200
MicroViaDrill 50
MicroViasAllowed 0
MicroViaMinSize 200
MicroViaMinDrill 50
TextPcbWidth 120
TextPcbSize 600 800
EdgeModWidth 150
TextModSize 600 600
TextModWidth 120
PadSize 808 808
PadDrill 591
Pad2MaskClearance 100
AuxiliaryAxisOrg 0 0
PcbPlotParams (pcbplotparams (layerselection 317751297) (usegerberextensions true) (excludeedgelayer true) (linewidth 60) (plotframeref false) (viasonmask true) (mode 1) (useauxorigin false) (hpglpennumber 1) (hpglpenspeed 20) (hpglpendiameter 15) (hpglpenoverlay 0) (pscolor true) (psnegative false) (psa4output false) (plotreference true) (plotvalue true) (plotothertext true) (plotinvisibletext false) (padsonsilk false) (subtractmaskfromsilk false) (outputformat 1) (mirror false) (drillshape 1) (scaleselection 1) (outputdirectory "E:/TSTx/Beta/TSTx v2/GERBER/"))
$EndSETUP

$EQUIPOT
Na 0 ""
St ~
$EndEQUIPOT
$EQUIPOT
Na 1 "+12V"
St ~
$EndEQUIPOT
$EQUIPOT
Na 2 "GND"
St ~
$EndEQUIPOT
$EQUIPOT
Na 3 "N-000001"
St ~
$EndEQUIPOT
$EQUIPOT
Na 4 "N-000003"
St ~
$EndEQUIPOT
$EQUIPOT
Na 5 "N-000004"
St ~
$EndEQUIPOT
$EQUIPOT
Na 6 "N-000006"
St ~
$EndEQUIPOT
$EQUIPOT
Na 7 "N-000007"
St ~
$EndEQUIPOT
$EQUIPOT
Na 8 "N-000008"
St ~
$EndEQUIPOT
$NCLASS
Name "Default"
Desc "To jest domyślna klasa połączeń."
Clearance 100
TrackWidth 98
ViaDia 350
ViaDrill 250
uViaDia 200
uViaDrill 50
AddNet ""
AddNet "+12V"
AddNet "GND"
AddNet "N-000001"
AddNet "N-000003"
AddNet "N-000004"
AddNet "N-000006"
AddNet "N-000007"
AddNet "N-000008"
$EndNCLASS
$MODULE PIN_ARRAY_3X1_C
Po 27100 9000 1800 15 5287F53B 51CB63F6 ~~
Li PIN_ARRAY_3X1_C
Cd Connecteur 3 pins
Kw CONN DEV
Sc 51CB63F6
AR /51CB60AD
Op 0 0 0
T0 100 -850 400 400 1800 60 N V 21 N "SW1"
T1 0 -850 400 400 1800 60 N I 21 N "BB"
DS 1650 -450 1650 550 60 21
DS 650 550 1650 550 60 21
DS 650 -550 1650 -550 60 21
DS 550 -450 550 550 60 21
DS -550 450 -550 -550 60 21
DS -1650 550 -1650 -450 60 21
DS -1650 450 -1650 -550 60 21
DS 550 -550 550 450 60 21
DS -550 550 -550 -450 60 21
DS -1650 -550 1350 -550 60 21
DS 1650 -550 1650 450 60 21
DS 1350 550 -1650 550 60 21
$PAD
Sh "1" C 689 689 0 0 1800
Dr 500 0 0
At STD N 00E0FFFF
Ne 8 "N-000008"
Po -1100 0
$EndPAD
$PAD
Sh "2" R 689 689 0 0 1800
Dr 500 0 0
At STD N 00E0FFFF
Ne 2 "GND"
Po 0 0
$EndPAD
$PAD
Sh "3" C 689 689 0 0 1800
Dr 500 0 0
At STD N 00E0FFFF
Ne 6 "N-000006"
Po 1100 0
$EndPAD
$SHAPE3D
Na "pin_array/pins_array_3x1.wrl"
Sc 1.000000 1.000000 1.000000
Of 0.000000 0.000000 0.000000
Ro 0.000000 0.000000 0.000000
$EndSHAPE3D
$EndMODULE  PIN_ARRAY_3X1_C
$MODULE PIN_ARRAY_3X1_FAR
Po 28000 16500 1800 15 5287F2B6 51C9C45B ~~
Li PIN_ARRAY_3X1_FAR
Cd Connecteur 3 pins far
Kw CONN DEV
Sc 51C9C45B
AR /51C9BEE5
Op 0 0 0
T0 100 -850 400 400 1800 60 N V 21 N "K2"
T1 0 -850 400 400 1800 60 N I 21 N "BUZ11"
DS -1500 -500 -1500 500 60 21
DS -500 -500 -500 500 60 21
DS 500 -500 500 500 60 21
DS 1500 -500 1500 500 60 21
DS 1500 500 2500 500 60 21
DS 2500 500 2500 -500 60 21
DS 1500 -500 2500 -500 60 21
DS -2500 -500 -1500 -500 60 21
DS -2500 500 -2500 -500 60 21
DS -1500 -500 1500 -500 60 21
DS 1500 500 -1500 500 60 21
DS -2500 500 -1500 500 60 21
$PAD
Sh "2" C 689 689 0 0 1800
Dr 500 0 0
At STD N 00E0FFFF
Ne 5 "N-000004"
Po 0 0
$EndPAD
$PAD
Sh "3" C 689 689 0 0 1800
Dr 500 0 0
At STD N 00E0FFFF
Ne 4 "N-000003"
Po 2000 0
$EndPAD
$PAD
Sh "1" C 689 689 0 0 1800
Dr 500 0 0
At STD N 00E0FFFF
Ne 2 "GND"
Po -2000 0
$EndPAD
$SHAPE3D
Na "pin_array/pins_array_3x1.wrl"
Sc 1.000000 1.000000 1.000000
Of 0.000000 0.000000 0.000000
Ro 0.000000 0.000000 0.000000
$EndSHAPE3D
$EndMODULE  PIN_ARRAY_3X1_FAR
$MODULE 1PIN_SQUARE
Po 32200 17700 0 15 5287CECB 51CB6971 ~~
Li 1PIN_SQUARE
Cd module 1 pin (ou trou mecanique de percage)
Kw DEV
Sc 51CB6971
AR /51CB3F06
Op 0 0 0
T0 0 -1200 400 400 0 100 N V 21 N "P1"
T1 0 1100 400 400 0 100 N I 21 N "12V"
DC 0 0 500 450 150 21
$PAD
Sh "1" R 808 808 0 0 0
Dr 591 0 0
At STD N 00E0FFFF
Ne 1 "+12V"
Po 0 0
$EndPAD
$EndMODULE  1PIN_SQUARE
$MODULE R3
Po 31200 9000 1800 15 51CB43E7 51C4B79A ~~
Li R3
Cd Resitance 3 pas
Kw R
Sc 51C4B79A
AR /51C49C8E
Op 0 A 0
T0 0 -1000 550 500 1800 80 N I 21 N "R1"
T1 0 50 550 500 1800 80 N V 21 N "10K"
DS -1500 0 -1300 0 80 21
DS 1500 0 1300 0 80 21
DS 1300 0 1300 -400 80 21
DS 1300 -400 -1300 -400 80 21
DS -1300 -400 -1300 400 80 21
DS -1300 400 1300 400 80 21
DS 1300 400 1300 0 80 21
DS -1300 -200 -1100 -400 80 21
$PAD
Sh "1" C 550 550 0 0 1800
Dr 320 0 0
At STD N 00E0FFFF
Ne 7 "N-000007"
Po -1500 0
$EndPAD
$PAD
Sh "2" C 550 550 0 0 1800
Dr 320 0 0
At STD N 00E0FFFF
Ne 8 "N-000008"
Po 1500 0
$EndPAD
$SHAPE3D
Na "discret/resistor.wrl"
Sc 0.300000 0.300000 0.300000
Of 0.000000 0.000000 0.000000
Ro 0.000000 0.000000 0.000000
$EndSHAPE3D
$EndMODULE  R3
$MODULE R3
Po 27500 15000 0 15 4E4C0E65 51C4B79C ~~
Li R3
Cd Resitance 3 pas
Kw R
Sc 51C4B79C
AR /51C4A9E2
Op 0 A 0
T0 0 50 550 500 0 80 N I 21 N "R2"
T1 0 50 550 500 0 80 N V 21 N "680"
DS -1500 0 -1300 0 80 21
DS 1500 0 1300 0 80 21
DS 1300 0 1300 -400 80 21
DS 1300 -400 -1300 -400 80 21
DS -1300 -400 -1300 400 80 21
DS -1300 400 1300 400 80 21
DS 1300 400 1300 0 80 21
DS -1300 -200 -1100 -400 80 21
$PAD
Sh "1" C 550 550 0 0 0
Dr 320 0 0
At STD N 00E0FFFF
Ne 4 "N-000003"
Po -1500 0
$EndPAD
$PAD
Sh "2" C 550 550 0 0 0
Dr 320 0 0
At STD N 00E0FFFF
Ne 3 "N-000001"
Po 1500 0
$EndPAD
$SHAPE3D
Na "discret/resistor.wrl"
Sc 0.300000 0.300000 0.300000
Of 0.000000 0.000000 0.000000
Ro 0.000000 0.000000 0.000000
$EndSHAPE3D
$EndMODULE  R3
$MODULE DIP-8__300
Po 27500 11500 1800 15 43A7F843 51C4B7A0 ~~
Li DIP-8__300
Cd 8 pins DIL package, round pads
Kw DIL
Sc 51C4B7A0
AR /51C49AE9
Op 0 0 0
T0 -2500 0 500 450 2700 80 N V 21 N "U1"
T1 0 0 500 400 1800 80 N V 21 N "PIC12F683"
DS -2000 -500 -1500 -500 100 21
DS -1500 -500 -1500 500 100 21
DS -1500 500 -2000 500 100 21
DS -2000 -1000 2000 -1000 100 21
DS 2000 -1000 2000 1000 100 21
DS 2000 1000 -2000 1000 100 21
DS -2000 1000 -2000 -1000 100 21
$PAD
Sh "1" R 550 550 0 0 1800
Dr 320 0 0
At STD N 00E0FFFF
Ne 7 "N-000007"
Po -1500 1500
$EndPAD
$PAD
Sh "2" C 550 550 0 0 1800
Dr 320 0 0
At STD N 00E0FFFF
Ne 8 "N-000008"
Po -500 1500
$EndPAD
$PAD
Sh "3" C 550 550 0 0 1800
Dr 320 0 0
At STD N 00E0FFFF
Ne 2 "GND"
Po 500 1500
$EndPAD
$PAD
Sh "4" C 550 550 0 0 1800
Dr 320 0 0
At STD N 00E0FFFF
Ne 6 "N-000006"
Po 1500 1500
$EndPAD
$PAD
Sh "5" C 550 550 0 0 1800
Dr 320 0 0
At STD N 00E0FFFF
Ne 3 "N-000001"
Po 1500 -1500
$EndPAD
$PAD
Sh "6" C 550 550 0 0 1800
Dr 320 0 0
At STD N 00E0FFFF
Ne 0 ""
Po 500 -1500
$EndPAD
$PAD
Sh "7" C 550 550 0 0 1800
Dr 320 0 0
At STD N 00E0FFFF
Ne 6 "N-000006"
Po -500 -1500
$EndPAD
$PAD
Sh "8" C 550 550 0 0 1800
Dr 320 0 0
At STD N 00E0FFFF
Ne 2 "GND"
Po -1500 -1500
$EndPAD
$SHAPE3D
Na "dil/dil_8.wrl"
Sc 1.000000 1.000000 1.000000
Of 0.000000 0.000000 0.000000
Ro 0.000000 0.000000 0.000000
$EndSHAPE3D
$EndMODULE  DIP-8__300
$MODULE C1V5
Po 32200 15900 1800 15 3E070CF4 51C4B7A1 ~~
Li C1V5
Cd Condensateur e = 1 pas
Kw C
Sc 51C4B7A1
AR /51C49C58
Op 0 0 0
T0 0 -499 300 300 1800 50 N V 21 N "C1"
T1 0 500 300 250 1800 50 N V 21 N "100nF"
T2 -900 0 300 300 1800 75 N V 21 N "+"
DC 0 0 50 -1000 50 21
$PAD
Sh "1" R 550 550 0 0 1800
Dr 320 0 0
At STD N 00E0FFFF
Ne 1 "+12V"
Po -500 0
$EndPAD
$PAD
Sh "2" C 550 550 0 0 1800
Dr 320 0 0
At STD N 00E0FFFF
Ne 2 "GND"
Po 500 0
$EndPAD
$SHAPE3D
Na "discret/c_vert_c1v5.wrl"
Sc 1.000000 1.000000 1.000000
Of 0.000000 0.000000 0.000000
Ro 0.000000 0.000000 0.000000
$EndSHAPE3D
$EndMODULE  C1V5
$MODULE R3
Po 27500 14000 0 15 51C9EC80 51C9C402 ~~
Li R3
Cd Resitance 3 pas
Kw R
Sc 51C9C402
AR /51C9C16E
Op 0 A 0
T0 0 -500 550 500 0 80 N I 21 N "R3"
T1 0 0 550 500 0 80 N V 21 N "100K"
DS -1500 0 -1300 0 80 21
DS 1500 0 1300 0 80 21
DS 1300 0 1300 -400 80 21
DS 1300 -400 -1300 -400 80 21
DS -1300 -400 -1300 400 80 21
DS -1300 400 1300 400 80 21
DS 1300 400 1300 0 80 21
DS -1300 -200 -1100 -400 80 21
$PAD
Sh "1" C 550 550 0 0 0
Dr 320 0 0
At STD N 00E0FFFF
Ne 4 "N-000003"
Po -1500 0
$EndPAD
$PAD
Sh "2" C 550 550 0 0 0
Dr 320 0 0
At STD N 00E0FFFF
Ne 2 "GND"
Po 1500 0
$EndPAD
$SHAPE3D
Na "discret/resistor.wrl"
Sc 0.300000 0.300000 0.300000
Of 0.000000 0.000000 0.000000
Ro 0.000000 0.000000 0.000000
$EndSHAPE3D
$EndMODULE  R3
$MODULE PIN_ARRAY_3X1_B
Po 30900 13000 900 15 51CDB090 51C4BEC6 ~~
Li PIN_ARRAY_3X1_B
Cd Connecteur 3 pins
Kw CONN DEV
Sc 51C4BEC6
AR /51C9BEB9
Op 0 0 0
T0 100 -850 400 400 900 60 N V 21 N "K1"
T1 0 -850 400 400 900 60 N I 21 N "78L05"
DS 500 500 500 -500 60 21
DS -1500 500 -1500 -500 60 21
DS -1500 -500 1500 -500 60 21
DS 1500 -500 1500 500 60 21
DS 1500 500 -1500 500 60 21
DS -500 -500 -500 500 60 21
$PAD
Sh "1" C 600 600 0 0 900
Dr 400 0 0
At STD N 00E0FFFF
Ne 1 "+12V"
Po -1000 0
$EndPAD
$PAD
Sh "2" R 600 600 0 0 900
Dr 400 0 0
At STD N 00E0FFFF
Ne 2 "GND"
Po 0 0
$EndPAD
$PAD
Sh "3" C 600 600 0 0 900
Dr 400 0 0
At STD N 00E0FFFF
Ne 7 "N-000007"
Po 1000 0
$EndPAD
$SHAPE3D
Na "pin_array/pins_array_3x1.wrl"
Sc 1.000000 1.000000 1.000000
Of 0.000000 0.000000 0.000000
Ro 0.000000 0.000000 0.000000
$EndSHAPE3D
$EndMODULE  PIN_ARRAY_3X1_B
$MODULE C1_6mm
Po 31500 10300 0 15 5287C7F2 51C4B7A4 ~~
Li C1_6mm
Cd Condensateur e = 1 pas
Kw C
Sc 51C4B7A4
AR /51C49C11
Op 0 0 0
T0 0 1000 400 400 0 80 N V 21 N "C3"
T1 0 -900 400 400 0 80 N I 21 N "100"
DS 1700 -500 -300 -500 120 21
DS 1700 500 -300 500 120 21
DS -1680 -500 300 -500 120 21
DS 1700 -500 1700 500 120 21
DS 300 500 -1700 500 120 21
DS -1700 500 -1700 -500 120 21
DS -1700 -250 -1450 -500 120 21
$PAD
Sh "1" C 550 550 0 0 0
Dr 320 0 0
At STD N 00E0FFFF
Ne 7 "N-000007"
Po -1200 0
$EndPAD
$PAD
Sh "2" C 550 550 0 0 0
Dr 320 0 0
At STD N 00E0FFFF
Ne 2 "GND"
Po 1200 0
$EndPAD
$SHAPE3D
Na "discret/capa_1_pas.wrl"
Sc 1.000000 1.000000 1.000000
Of 0.000000 0.000000 0.000000
Ro 0.000000 0.000000 0.000000
$EndSHAPE3D
$EndMODULE  C1_6mm
$MODULE C1_6mm
Po 32700 12900 900 15 5287C7F2 51C4B7A2 ~~
Li C1_6mm
Cd Condensateur e = 1 pas
Kw C
Sc 51C4B7A2
AR /51C49C1E
Op 0 0 0
T0 0 1000 400 400 900 80 N V 21 N "C2"
T1 0 -900 400 400 900 80 N I 21 N "100"
DS 1700 -500 -300 -500 120 21
DS 1700 500 -300 500 120 21
DS -1680 -500 300 -500 120 21
DS 1700 -500 1700 500 120 21
DS 300 500 -1700 500 120 21
DS -1700 500 -1700 -500 120 21
DS -1700 -250 -1450 -500 120 21
$PAD
Sh "1" C 550 550 0 0 900
Dr 320 0 0
At STD N 00E0FFFF
Ne 1 "+12V"
Po -1200 0
$EndPAD
$PAD
Sh "2" C 550 550 0 0 900
Dr 320 0 0
At STD N 00E0FFFF
Ne 2 "GND"
Po 1200 0
$EndPAD
$SHAPE3D
Na "discret/capa_1_pas.wrl"
Sc 1.000000 1.000000 1.000000
Of 0.000000 0.000000 0.000000
Ro 0.000000 0.000000 0.000000
$EndSHAPE3D
$EndMODULE  C1_6mm
$MODULE 1PIN_SQUARE
Po 30000 17700 0 15 528B0868 528B07B4 ~~
Li 1PIN_SQUARE
Cd module 1 pin (ou trou mecanique de percage)
Kw DEV
Sc 528B07B4
AR /51CB3F25
Op 0 0 0
T0 0 -1200 400 400 0 100 N V 21 N "P2"
T1 0 1100 400 400 0 100 N I 21 N "GND"
DC 0 0 500 450 150 21
$PAD
Sh "1" R 808 808 0 0 0
Dr 591 0 0
At STD N 00E0FFFF
Ne 2 "GND"
Po 0 0
$EndPAD
$EndMODULE  1PIN_SQUARE
$MODULE 1PIN_SQUARE
Po 28000 17700 0 15 528B0868 528B07B6 ~~
Li 1PIN_SQUARE
Cd module 1 pin (ou trou mecanique de percage)
Kw DEV
Sc 528B07B6
AR /51CB3DDC
Op 0 0 0
T0 0 -1200 400 400 0 100 N V 21 N "P3"
T1 0 1100 400 400 0 100 N I 21 N "GRZ"
DC 0 0 500 450 150 21
$PAD
Sh "1" R 808 808 0 0 0
Dr 591 0 0
At STD N 00E0FFFF
Ne 5 "N-000004"
Po 0 0
$EndPAD
$EndMODULE  1PIN_SQUARE
$COTATION
Ge 0 25 0
Va 10400
Te "26,416 mm"
Po 23661 13200 600 800 120 2700 1
Sb 0 24301 8000 24301 18400 120
Sd 0 24600 18400 23021 18400 120
Sg 0 24600 8000 23021 8000 120
S1 0 24301 18400 24071 17957 120
S2 0 24301 18400 24531 17957 120
S3 0 24301 8000 24071 8443 120
S4 0 24301 8000 24531 8443 120
$endCOTATION
$COTATION
Ge 0 25 0
Va 8600
Te "21,844 mm"
Po 29300 19739 600 800 120 0 1
Sb 0 25000 19099 33600 19099 120
Sd 0 33600 18800 33600 20379 120
Sg 0 25000 18800 25000 20379 120
S1 0 33600 19099 33157 19329 120
S2 0 33600 19099 33157 18869 120
S3 0 25000 19099 25443 19329 120
S4 0 25000 19099 25443 18869 120
$endCOTATION
$DRAWSEGMENT
Po 0 33600 18400 33600 8000 150
De 28 0 900 0 0
$EndDRAWSEGMENT
$DRAWSEGMENT
Po 0 25000 8000 25000 18400 150
De 28 0 900 0 0
$EndDRAWSEGMENT
$DRAWSEGMENT
Po 0 25050 8000 33550 8000 150
De 28 0 900 0 0
$EndDRAWSEGMENT
$DRAWSEGMENT
Po 0 25050 18450 33550 18450 150
De 28 0 900 0 0
$EndDRAWSEGMENT
$TRACK
Po 0 25300 12000 25300 11500 102 -1
De 0 0 0 0 0
Po 0 25700 11800 25700 12000 102 -1
De 0 0 0 0 0
Po 0 25700 12000 25500 12200 102 -1
De 0 0 0 0 0
Po 0 25300 12000 25500 12200 102 -1
De 0 0 0 0 0
Po 0 25900 12200 25700 12000 102 -1
De 0 0 0 0 0
Po 0 26100 12000 25900 12200 102 -1
De 0 0 0 0 0
Po 0 26100 11500 26100 12000 102 -1
De 0 0 0 0 0
Po 0 32700 15900 32700 17200 591 -1
De 0 0 1 0 400000
Po 0 32700 17200 32200 17700 591 -1
De 0 0 1 0 800000
Po 0 32600 14000 32700 14100 591 -1
De 0 0 1 0 800000
Po 0 32700 15900 32700 14100 591 -1
De 0 0 1 0 C00000
Po 0 30900 14000 32600 14000 591 -1
De 0 0 1 0 400000
Po 0 30500 13000 29000 13000 591 -1
De 0 0 2 0 800000
Po 0 27000 9100 27100 9000 394 -1
De 0 0 2 0 800000
Po 0 31400 13000 32700 11700 394 -1
De 0 0 2 0 800000
Po 0 27000 10000 27000 9100 394 -1
De 0 0 2 0 400000
Po 0 32700 11700 32700 10300 394 -1
De 0 0 2 0 C00000
Po 0 29000 14000 30000 15000 394 -1
De 0 0 2 0 400000
Po 0 31700 15900 30100 15900 591 -1
De 0 0 2 0 400000
Po 0 29000 12000 29000 13000 394 -1
De 0 0 2 0 800000
Po 0 27000 10000 29000 12000 394 -1
De 0 0 2 0 400000
Po 0 30000 16000 30000 16500 591 -1
De 0 0 2 0 800000
Po 0 30000 15000 30000 16000 591 -1
De 0 0 2 0 0
Po 0 30100 15900 30000 16000 591 -1
De 0 0 2 0 0
Po 0 30900 13000 31400 13000 394 -1
De 0 0 2 0 400000
Po 0 29000 13000 29000 14000 394 -1
De 0 0 2 0 C00000
Po 0 28000 15000 26000 13000 394 -1
De 0 0 3 0 800000
Po 0 28000 15000 28500 15000 394 -1
De 0 0 3 0 0
Po 0 29000 15000 28500 15000 394 -1
De 0 0 3 0 400000
Po 0 26000 16500 26000 16000 394 -1
De 0 0 4 0 400000
Po 0 26000 15000 26000 16500 394 -1
De 0 0 4 0 C00000
Po 0 26000 14000 26000 15000 394 -1
De 0 0 4 0 C00000
Po 0 26000 10000 26000 10400 394 -1
De 0 0 6 0 400000
Po 0 26000 10000 26000 9000 394 -1
De 0 0 6 0 C00000
Po 0 26000 10400 28000 12400 394 -1
De 0 0 6 0 0
Po 0 28000 12400 28000 13000 394 -1
De 0 0 6 0 800000
Po 0 30800 10300 32100 9000 394 -1
De 0 0 7 0 0
Po 0 30300 10300 29300 10300 394 -1
De 0 0 7 0 400000
Po 0 32100 9000 32700 9000 394 -1
De 0 0 7 0 800000
Po 0 30300 10300 30800 10300 394 -1
De 0 0 7 0 400000
Po 0 30900 10400 30800 10300 394 -1
De 0 0 7 0 0
Po 0 30900 12000 30900 10400 394 -1
De 0 0 7 0 400000
Po 0 29300 10300 29000 10000 394 -1
De 0 0 7 0 800000
Po 0 28200 9000 29700 9000 394 -1
De 0 0 8 0 C00000
Po 0 28000 10000 28000 9200 394 -1
De 0 0 8 0 400000
Po 0 28000 9200 28200 9000 394 -1
De 0 0 8 0 800000
$EndTRACK
$ZONE
$EndZONE
$CZONE_OUTLINE
ZInfo 51CD7E4E 4 "N-000003"
ZLayer 0
ZAux 4 E
ZClearance 0 T
ZMinThickness 100
ZOptions 0 16 F 200 200
ZSmoothing 0 0
ZCorner 26900 17300 0
ZCorner 26900 15700 0
ZCorner 25100 15700 0
ZCorner 25100 17300 1
$POLYSCORNERS
26850 17250 0 0
26543 17250 0 0
26543 16579 0 0
26532 16366 0 0
26472 16219 0 0
26378 16192 0 0
26308 16262 0 0
26308 16122 0 0
26281 16028 0 0
26079 15957 0 0
25866 15968 0 0
25719 16028 0 0
25692 16122 0 0
26000 16429 0 0
26308 16122 0 0
26308 16262 0 0
26071 16500 0 0
26378 16808 0 0
26472 16781 0 0
26543 16579 0 0
26543 17250 0 0
26308 17250 0 0
26308 16878 0 0
26000 16571 0 0
25929 16641 0 0
25929 16500 0 0
25622 16192 0 0
25528 16219 0 0
25457 16421 0 0
25468 16634 0 0
25528 16781 0 0
25622 16808 0 0
25929 16500 0 0
25929 16641 0 0
25692 16878 0 0
25719 16972 0 0
25921 17043 0 0
26134 17032 0 0
26281 16972 0 0
26308 16878 0 0
26308 17250 0 0
25150 17250 0 0
25150 15750 0 0
26850 15750 0 0
26850 17250 1 0
$endPOLYSCORNERS
$endCZONE_OUTLINE
$CZONE_OUTLINE
ZInfo 51D1B087 0 ""
ZLayer 22
ZAux 6 E
ZClearance 0 T
ZMinThickness 100
ZOptions 0 16 F 200 200
ZSmoothing 0 0
ZCorner 25000 18500 0
ZCorner 33600 18400 0
ZCorner 33600 17000 0
ZCorner 31000 17000 0
ZCorner 31000 15700 0
ZCorner 25000 15700 1
$POLYSCORNERS
25000 18500 0 0
33600 18400 0 0
33600 17000 0 0
31000 17000 0 0
31000 15700 0 0
25000 15700 1 0
$endPOLYSCORNERS
$endCZONE_OUTLINE
$CZONE_OUTLINE
ZInfo 51CD7DE1 5 "N-000004"
ZLayer 0
ZAux 4 E
ZClearance 0 T
ZMinThickness 100
ZOptions 0 16 F 200 200
ZSmoothing 0 0
ZCorner 28900 18500 0
ZCorner 28900 15700 0
ZCorner 27100 15700 0
ZCorner 27100 18500 1
$POLYSCORNERS
28850 18325 0 0
28587 18325 0 0
28587 16589 0 0
28576 16358 0 0
28508 16193 0 0
28409 16161 0 0
28339 16231 0 0
28339 16091 0 0
28307 15992 0 0
28089 15913 0 0
27858 15924 0 0
27693 15992 0 0
27661 16091 0 0
28000 16429 0 0
28339 16091 0 0
28339 16231 0 0
28071 16500 0 0
28409 16839 0 0
28508 16807 0 0
28587 16589 0 0
28587 18325 0 0
28339 18325 0 0
28339 16909 0 0
28000 16571 0 0
27929 16641 0 0
27929 16500 0 0
27591 16161 0 0
27492 16193 0 0
27413 16411 0 0
27424 16642 0 0
27492 16807 0 0
27591 16839 0 0
27929 16500 0 0
27929 16641 0 0
27661 16909 0 0
27693 17008 0 0
27911 17087 0 0
28142 17076 0 0
28307 17008 0 0
28339 16909 0 0
28339 18325 0 0
27150 18325 0 0
27150 15750 0 0
28850 15750 0 0
28850 18325 1 0
$endPOLYSCORNERS
$endCZONE_OUTLINE
$CZONE_OUTLINE
ZInfo 51CD7C60 1 "+12V"
ZLayer 0
ZAux 4 E
ZClearance 0 T
ZMinThickness 100
ZOptions 0 16 F 200 200
ZSmoothing 0 0
ZCorner 33200 18400 0
ZCorner 33200 17000 0
ZCorner 31200 17000 0
ZCorner 31200 18400 1
$POLYSCORNERS
33150 18325 0 0
32720 18325 0 0
32745 18315 0 0
32815 18245 0 0
32853 18154 0 0
32853 18055 0 0
32854 17812 0 0
32792 17750 0 0
32300 17750 0 0
32250 17750 0 0
32150 17750 0 0
32100 17750 0 0
31608 17750 0 0
31546 17812 0 0
31547 18055 0 0
31547 18154 0 0
31585 18245 0 0
31655 18315 0 0
31679 18325 0 0
31250 18325 0 0
31250 17050 0 0
31739 17050 0 0
31655 17085 0 0
31585 17155 0 0
31547 17246 0 0
31547 17345 0 0
31546 17588 0 0
31608 17650 0 0
32100 17650 0 0
32150 17650 0 0
32250 17650 0 0
32300 17650 0 0
32792 17650 0 0
32854 17588 0 0
32853 17345 0 0
32853 17246 0 0
32815 17155 0 0
32745 17085 0 0
32660 17050 0 0
33150 17050 0 0
33150 18325 1 0
$endPOLYSCORNERS
$endCZONE_OUTLINE
$CZONE_OUTLINE
ZInfo 5287F3F3 2 "GND"
ZLayer 0
ZAux 4 E
ZClearance 0 T
ZMinThickness 100
ZOptions 0 16 F 200 200
ZSmoothing 0 0
ZCorner 31000 18400 0
ZCorner 31000 15700 0
ZCorner 29100 15700 0
ZCorner 29100 18400 1
$POLYSCORNERS
30950 18325 0 0
30587 18325 0 0
30587 16589 0 0
30576 16358 0 0
30508 16193 0 0
30409 16161 0 0
30339 16231 0 0
30339 16091 0 0
30307 15992 0 0
30089 15913 0 0
29858 15924 0 0
29693 15992 0 0
29661 16091 0 0
30000 16429 0 0
30339 16091 0 0
30339 16231 0 0
30071 16500 0 0
30409 16839 0 0
30508 16807 0 0
30587 16589 0 0
30587 18325 0 0
30339 18325 0 0
30339 16909 0 0
30000 16571 0 0
29929 16641 0 0
29929 16500 0 0
29591 16161 0 0
29492 16193 0 0
29413 16411 0 0
29424 16642 0 0
29492 16807 0 0
29591 16839 0 0
29929 16500 0 0
29929 16641 0 0
29661 16909 0 0
29693 17008 0 0
29911 17087 0 0
30142 17076 0 0
30307 17008 0 0
30339 16909 0 0
30339 18325 0 0
29150 18325 0 0
29150 15750 0 0
30950 15750 0 0
30950 18325 1 0
$endPOLYSCORNERS
$endCZONE_OUTLINE
$EndBOARD
